**Mid-Bass speaker B4N**

|  |
| --- |
| 4” |
|  |
| 3.5” |
|  |
| 3” |
|  |
| 1.5”  |
|  |
| 0” |
|  |
|  |
|  | **Specification****Rated Impedance 8ohm****Resonant Frequency 56H z****Rated Power 25W****Max Power 50W****Sensitivity2.83v/1m） 85dB****Coil diameter 25mm****Coil Roll With 10.4mm****DC resistance 6.5ohm****coil wire High temp.SV wire****Coil frame High tem. Kapton****Magnet High per. ferrite****Force coefficient 5.1N/A****Magnetic gap height 4.0mm****Xmax 3.2mm****Compliance 1114.1uM/N****Mechanical Q value 3.91 -****Electric Q value 063 -****Total Q value 0.52 -****Vibration Quality 6.8g****Equivalent volume 4.5L****SD(cm²) 52,81****Cabinet type Inverted****Free Volume 5L****Frequency Field -3db Frequency 50Hz** |
|  |
|  |