**Mid-Bass speaker B4N**

|  |  |
| --- | --- |
| 4” | |
|  | |
| 3.5” | |
|  | |
| 3” | |
|  | |
| 1.5” | |
|  | |
| 0” | |
|  | |
|  | |
|  | **Specification**  **Rated Impedance 8ohm**  **Resonant Frequency 56H z**  **Rated Power 25W**  **Max Power 50W**  **Sensitivity2.83v/1m） 85dB**  **Coil diameter 25mm**  **Coil Roll With 10.4mm**  **DC resistance 6.5ohm**  **coil wire High temp.SV wire**  **Coil frame High tem. Kapton**  **Magnet High per. ferrite**  **Force coefficient 5.1N/A**  **Magnetic gap height 4.0mm**  **Xmax 3.2mm**  **Compliance 1114.1uM/N**  **Mechanical Q value 3.91 -**  **Electric Q value 063 -**  **Total Q value 0.52 -**  **Vibration Quality 6.8g**  **Equivalent volume 4.5L**  **SD(cm²) 52,81**  **Cabinet type Inverted**  **Free Volume 5L**  **Frequency Field -3db Frequency 50Hz** |
|  |
|  |