**full-range speaker B2S**

|  |  |
| --- | --- |
| 2” 2” | |
|  | |
| 1.5” 1.5” | |
|  | |
| 1” 1” | |
|  | |
| 0.5” 0.5” | |
|  | |
| 0” | |
|  | |
|  | |
|  | **Specification**  **Rated Impedance 8Ω**  **Resonance Frequency 152Hz**  **Rated Power 10W**  **Peak Power 20W**  **Sensitivity(2.83V/1m) 78dB**  **Weight 0.12kg**  **Diameter 25mm**  **DC Resistance 6.5Ω**  **Width 6.0mm**  **Coil wire CCAW**  **Frame Kapton**  **Material Ferrite**  **BL Value 2.5 N/A**  **Magnetic gap height 3.0mm**  **Xmax 1.5mm**  **Compliance 689uM/N**  **QMS 5.69**  **QES 1.53**  **Qts 1.2**  **Mms**  **Vas 0.2L**  **SD(cm²) 13,53**  **Recommend Cabinet**  **Closed** |
|  |
|  |