**full-range speaker B2S**

|  |
| --- |
| 2” 2” |
|  |
| 1.5” 1.5” |
|  |
| 1” 1” |
|  |
| 0.5” 0.5” |
|  |
| 0” |
|  |
|  |
|  | **Specification** **Rated Impedance 8Ω****Resonance Frequency 152Hz****Rated Power 10W****Peak Power 20W****Sensitivity(2.83V/1m) 78dB****Weight 0.12kg****Diameter 25mm****DC Resistance 6.5Ω****Width 6.0mm****Coil wire CCAW****Frame Kapton****Material Ferrite****BL Value 2.5 N/A****Magnetic gap height 3.0mm****Xmax 1.5mm****Compliance 689uM/N****QMS 5.69****QES 1.53****Qts 1.2****Mms** **Vas 0.2L****SD(cm²) 13,53****Recommend Cabinet****Closed** |
|  |
|  |