**Mid-bass speaker M5N**

|  |  |
| --- | --- |
| 5” | |
|  | |
| 4” | |
|  | |
| 3” | |
|  | |
| 2” | |
|  | |
| 0” | |
|  | |
|  | |
|  | **Specification**  **Rated Impedance 8ohm**  **Resonant Frequency 47H z**  **Rated Power 35W**  **Max Power 70W**  **Sensitivity2.83v/1m） 87dB**  **Coil diameter 25mm**  **Coil Roll With 10.5mm**  **DC resistance 6.5ohm**  **coil wire High temp. SV wire**  **Coil frame High temp. Kapton**  **Magnet High perfor. ferrite**  **Force coefficient 7.5N/A**  **Magnetic gap height 5.0mm**  **Xmax 2.7mm**  **Compliance 1051uM/N**  **Mechanical Q value 6.51 -**  **Electric Q value 0.37 -**  **Total Q value 0.35 -**  **Vibration Quality 10.7g**  **Equivalent volume 11.3L**  **SD(cm²) 86,59**  **Cabinet type Inverted**  **Free Volume 10L**  **Frequency Field -3db Frequency 48Hz** |