**full-range speaker B3S**

|  |
| --- |
| 3” |
|  |
| 2.5” |
|  |
| 2” |
|  |
| 1.5”  |
|  |
| 0” |
|  |
|  |
|  | **Specification****Rated Impedance 8ohm****Resonant Frequency 80Hz****Rated Power 15W****Max Power 30W****Sensitivity(2.83v/1m） 82dB****Coil diameter 25mm****Coil Roll With 9.0mm****DC resistance 6.5ohm****coil wire CCAW wire****Coil frame Kapton****Magnet High ferrite****Force coefficient 2.9N/A****Magnetic gap height 3.0mm****Xmax 3.0mm****Compliance 1260uM/N****Mechanical Q value 4.29 -****Electric Q value 1.19 -****Total Q value 0.93-****Vibration Quality 3.1g****Equivalent volume 1.6L****Cabinet type Closed****Free Volume 2L****SD(cm²) 29,22****Frequency Field -3db Frequency 80Hz** |
|  |
|  |