**full-range speaker B3S**

|  |  |
| --- | --- |
| 3” | |
|  | |
| 2.5” | |
|  | |
| 2” | |
|  | |
| 1.5” | |
|  | |
| 0” | |
|  | |
|  | |
|  | **Specification**  **Rated Impedance 8ohm**  **Resonant Frequency 80Hz**  **Rated Power 15W**  **Max Power 30W**  **Sensitivity(2.83v/1m） 82dB**  **Coil diameter 25mm**  **Coil Roll With 9.0mm**  **DC resistance 6.5ohm**  **coil wire CCAW wire**  **Coil frame Kapton**  **Magnet High ferrite**  **Force coefficient 2.9N/A**  **Magnetic gap height 3.0mm**  **Xmax 3.0mm**  **Compliance 1260uM/N**  **Mechanical Q value 4.29 -**  **Electric Q value 1.19 -**  **Total Q value 0.93-**  **Vibration Quality 3.1g**  **Equivalent volume 1.6L**  **Cabinet type Closed**  **Free Volume 2L**  **SD(cm²) 29,22**  **Frequency Field -3db Frequency 80Hz** |
|  |
|  |