**Mid-bass speaker L6-4R**

|  |  |
| --- | --- |
| 6” | |
|  | |
| 5” | |
|  | |
| 4” | |
|  | |
| 2” | |
|  | |
| 0” | |
|  | |
|  | **Specification**  **Rated Impedance 4ohm**  **Resonant Frequency 50H z**  **Rated Power 30W**  **Max Power 60W**  **Sensitivity2.83v/1m） 88dB**  **Coil diameter 30mm**  **Coil Roll With 14.6mm**  **DC resistance 3.6ohm**  **coil wire High temp. SV wire**  **Coil frame High temp. Kapton**  **Magnet High perf. ferrite**  **Force coefficient 6.0N/A**  **Magnetic gap height 6.0mm**  **Xmax 4.3mm**  **Compliance 588uM/N**  **Mechanical Q value 3.856-**  **Electric Q value 0.44 -**  **Total Q value 0.4 -**  **Vibration Quality 17.3g**  **Equivalent volume 14.7L**  **Cabinet type Inverted** |

