**Isodynamic Planar Tweeter RT1C-A**

|  |  |
| --- | --- |
| 4” | |
|  | |
| 3” | |
|  | |
| 2” | |
|  | |
| 1” | |
|  | |
| 0” | |
|  | |
|  | **An identifying mark:**  **Rated Impedance 5ohm**    **Rated Power 15W**  **Max Power 30W**  **Sensitivity(2.83v/1m） 94dB**  **Coil frame Isodynamic Ribbon**    **Magnet Neodymium bar matrix**  **Suggested Crossover >4500Hz** |

