**Tweeter Driver Q1R**

|  |  |
| --- | --- |
| 4” | |
|  | |
| 3” | |
|  | |
| 2” | |
|  | |
| 1” | |
|  | |
| 0” | |
|  | |
|  | **An identifying mark:**  **Rated Impedance 6ohm**  **Resonant Frequency**  **1000H z**  **Rated Power 15W**  **Max Power 30W**  **Sensitivity(2.83v/1m） 89dB**  **Coil diameter 28mm**  **DC resistance 5.3ohm**  **coil wire CCAW wire**  **Coil frame High temperature resistant AL**  **Magnetic circuit Shielded anti-magnetic magnetic circult**  **Magnet High perf. ferrite**  **Suggested Crossover >2500Hz** |

