**Mid-bass speaker M8N-1B**

|  |
| --- |
| 8” |
|  |
| 7” |
|  |
| 6” |
|  |
| 5” |
|  |
| 4” |
|  |
|  |
|  | **Specification** **Rated Impedance 8Ω****Resonance Frequency 29Hz****Rated Power 80W****Peak Power 160W****Sensitivity(2.83V/1m) 88dB****Weight 2.3kg****Diameter 35mm****DC Resistance 6.5Ω****Width 17.5mm****Fromer SV****Frame Kapton****Category External****Material Ferrite****BL Value 9.6 N/A****Magnetic gap height 6.0mm****Xmax 5.8mm****Complience 822uM/N****QMS 5.02****QES 0.5****Qts 0.45****Mms 36.5g****Vas 53.5L****SD(cm²) 208,67****Recommend Cabinet****Type Inverted type****Vb 22L****FB 34Hz****F3 40Hz** |
|  |
|  |