**Mid-bass speaker M8N-1B**

|  |  |
| --- | --- |
| 8” | |
|  | |
| 7” | |
|  | |
| 6” | |
|  | |
| 5” | |
|  | |
| 4” | |
|  | |
|  | |
|  | **Specification**  **Rated Impedance 8Ω**  **Resonance Frequency 29Hz**  **Rated Power 80W**  **Peak Power 160W**  **Sensitivity(2.83V/1m) 88dB**  **Weight 2.3kg**  **Diameter 35mm**  **DC Resistance 6.5Ω**  **Width 17.5mm**  **Fromer SV**  **Frame Kapton**  **Category External**  **Material Ferrite**  **BL Value 9.6 N/A**  **Magnetic gap height 6.0mm**  **Xmax 5.8mm**  **Complience 822uM/N**  **QMS 5.02**  **QES 0.5**  **Qts 0.45**  **Mms 36.5g**  **Vas 53.5L**  **SD(cm²) 208,67**  **Recommend Cabinet**  **Type Inverted type**  **Vb 22L**  **FB 34Hz**  **F3 40Hz** |
|  |
|  |