**Dome Tweeter Driver K1**

|  |
| --- |
| 3” |
|  |
|  |
|  |
| 2”  |
|  |
|   |
|  |
| 0” |
|  |
|   | **An identifying mark:****Rated Impedance 5ohm****Resonant Frequency 800H z****Rated Power 15W****Max Power 30W****Sensitivity2.83v/1m） 92dB****Coil diameter 25mm****DC resistance 4.6ohm****Coil wire High temperature resistant CCAW****Coil frame High temperature resistant AL****Magnet High performance ferrite****Suggested Crossover >2500Hz** |

