**Dome Tweeter Driver TN25**

|  |
| --- |
| 2” |
|  |
| 1.5” |
|  |
| 1”  |
|  |
|  0.5”  |
|  |
| 0”  |
|  |
|   | **An identifying mark:****Rated Impedance 5ohm****Resonant Frequency 1500H z****Rated Power 15W****Max Power 30W****Sensitivity(2.83v/1m） 90dB****Coil diameter 25mm****DC resistance 4.6ohm****coil wire CCAW wire****Coil frame High temperature resistant AL****Magnetic circuit Shielded anti-magnetic magnetic circult****Magnet High perf. ferrite****Suggested Crossover >2000Hz** |