**Mid-range Driver DMA-A**

|  |
| --- |
| 4” |
|  |
| 3” |
|  |
| 2”  |
|  |
| 1”  |
|  |
| 0”  |
|  |
|   | **An identifying mark:****Rated Impedance 5ohm****Resonant Frequency 630Hz****Rated Power 80W****Max Power 150W****Sensitivity（2.83v/1m） 92dB****Coil diameter 50mm****DC resistance 4.3ohm****coil wire High temperature resistant SV wire****Coil frame High temperature resistant AL****Magnetic circuit External magnetic circuit****Magnet High performance ferrite****Suggested Crossover >800Hz,<6000HZ** |

