**Mid-range Driver DMA-A**

|  |  |
| --- | --- |
| 4” | |
|  | |
| 3” | |
|  | |
| 2” | |
|  | |
| 1” | |
|  | |
| 0” | |
|  | |
|  | **An identifying mark:**  **Rated Impedance 5ohm**  **Resonant Frequency 630Hz**  **Rated Power 80W**  **Max Power 150W**  **Sensitivity（2.83v/1m） 92dB**  **Coil diameter 50mm**  **DC resistance 4.3ohm**  **coil wire High temperature resistant SV wire**  **Coil frame High temperature resistant AL**  **Magnetic circuit External magnetic circuit**  **Magnet High performance ferrite**  **Suggested Crossover >800Hz,<6000HZ** |

