**Mid-bass speaker M5N**

|  |
| --- |
| 5” |
|  |
| 4” |
|  |
| 3” |
|  |
| 2”  |
|  |
| 0” |
|  |
|  |
|   | **Specification****Rated Impedance 8ohm****Resonant Frequency 47H z****Rated Power 35W****Max Power 70W****Sensitivity2.83v/1m） 87dB****Coil diameter 25mm****Coil Roll With 10.5mm****DC resistance 6.5ohm****coil wire High temp. SV wire****Coil frame High temp. Kapton****Magnet High perfor. ferrite****Force coefficient 7.5N/A****Magnetic gap height 5.0mm****Xmax 2.7mm****Compliance 1051uM/N****Mechanical Q value 6.51 -****Electric Q value 0.37 -****Total Q value 0.35 -****Vibration Quality 10.7g****Equivalent volume 11.3L****SD(cm²) 86,59****Cabinet type Inverted****Free Volume 10L****Frequency Field -3db Frequency 48Hz** |