**Mid-bass speaker L6-4R**

|  |
| --- |
| 6” |
|  |
| 5” |
|  |
| 4”  |
|  |
| 2”  |
|  |
| 0” |
|  |
|   | **Specification****Rated Impedance 4ohm****Resonant Frequency 50H z****Rated Power 30W****Max Power 60W****Sensitivity2.83v/1m） 88dB****Coil diameter 30mm****Coil Roll With 14.6mm****DC resistance 3.6ohm****coil wire High temp. SV wire****Coil frame High temp. Kapton****Magnet High perf. ferrite****Force coefficient 6.0N/A****Magnetic gap height 6.0mm****Xmax 4.3mm****Compliance 588uM/N****Mechanical Q value 3.856-****Electric Q value 0.44 -****Total Q value 0.4 -****Vibration Quality 17.3g****Equivalent volume 14.7L****Cabinet type Inverted** |

