**Isodynamic Planar Tweeter RT1C-A**

|  |
| --- |
| 4” |
|  |
| 3” |
|  |
| 2”  |
|  |
|  1”  |
|  |
| 0”  |
|  |
|   | **An identifying mark:****Rated Impedance 5ohm****Rated Power 15W****Max Power 30W****Sensitivity(2.83v/1m） 94dB****Coil frame Isodynamic Ribbon****Magnet Neodymium bar matrix****Suggested Crossover >4500Hz** |

