**Tweeter Driver Q1R**

|  |
| --- |
| 4” |
|  |
| 3” |
|  |
| 2”  |
|  |
|  1” |
|  |
| 0”  |
|  |
|   | **An identifying mark:****Rated Impedance 6ohm****Resonant Frequency** **1000H z****Rated Power 15W****Max Power 30W****Sensitivity(2.83v/1m） 89dB****Coil diameter 28mm****DC resistance 5.3ohm****coil wire CCAW wire****Coil frame High temperature resistant AL****Magnetic circuit Shielded anti-magnetic magnetic circult****Magnet High perf. ferrite****Suggested Crossover >2500Hz** |

