**Dome Tweeter Driver K1**

|  |  |
| --- | --- |
| 3” | |
|  | |
|  | |
|  | |
| 2” | |
|  | |
|  | |
|  | |
| 0” | |
|  | |
|  | **An identifying mark:**  **Rated Impedance 5ohm**  **Resonant Frequency 800H z**  **Rated Power 15W**  **Max Power 30W**  **Sensitivity2.83v/1m） 92dB**  **Coil diameter 25mm**  **DC resistance 4.6ohm**  **Coil wire High temperature resistant CCAW**  **Coil frame High temperature resistant AL**  **Magnet High performance ferrite**  **Suggested Crossover >2500Hz** |

