**Mid-bass speaker D6.8B**

|  |  |
| --- | --- |
| 6” | |
|  | |
| 5” | |
|  | |
| 4” | |
|  | |
| 2” | |
|  | |
| 0” | |
|  | |
|  | **An identifying mark:**  **Rated Impedance 8ohm**  **Resonant Frequency 43H z**  **Rated Power 60W**  **Max Power 120W**  **Sensitivity(2.83v/1m） 85dB**  **Coil diameter 76mm**  **Coil Roll With 15.5mm**  **DC resistance 6.5ohm**  **coil wire CCAW**  **Coil frame High temp. Kapton**  **Magnet High perf. NdFeB**  **Force coefficient 8.9N/A**  **Magnetic gap height 5.0mm**  **Xmax 5.3mm**  **Compliance 647uM/N**  **Mechanical Q value 5.21 -**  **Electric Q value 0.49 -**  **Total Q value 0.45 -**  **Vibration Quality 21.9g**  **Equivalent volume 13.5L**  **SD(cm²) 120,76**  **Cabinet type Inverted**  **Free Volume 10L**  **Frequency Field -3db Frequency 44Hz** |