**Mid-bass speaker D6.8B**

|  |
| --- |
| 6” |
|  |
| 5” |
|  |
| 4”  |
|  |
| 2”  |
|  |
| 0” |
|  |
|   | **An identifying mark:****Rated Impedance 8ohm****Resonant Frequency 43H z****Rated Power 60W****Max Power 120W****Sensitivity(2.83v/1m） 85dB****Coil diameter 76mm****Coil Roll With 15.5mm****DC resistance 6.5ohm****coil wire CCAW****Coil frame High temp. Kapton****Magnet High perf. NdFeB****Force coefficient 8.9N/A****Magnetic gap height 5.0mm****Xmax 5.3mm****Compliance 647uM/N****Mechanical Q value 5.21 -****Electric Q value 0.49 -****Total Q value 0.45 -****Vibration Quality 21.9g****Equivalent volume 13.5L****SD(cm²) 120,76****Cabinet type Inverted****Free Volume 10L****Frequency Field -3db Frequency 44Hz** |