**Isodynamic Planar Tweeter RT1.3WE**

|  |
| --- |
| 4” |
|  |
| 3” |
|  |
| 2”  |
|  |
|  1”  |
|  |
| 0”  |
|  |
|   | **An identifying mark:****Rated Impedance 6ohm****Resonant Frequency** **1000H z****Rated Power 10W****Max Power 30W****Sensitivity(2.83v/1m） 92dB****DC resistance 5.4ohm****Magnet Neodymium****Suggested Crossover >2500Hz** |

