**Isodynamic Planar Tweeter RT1.3WE**

|  |  |
| --- | --- |
| 4” | |
|  | |
| 3” | |
|  | |
| 2” | |
|  | |
| 1” | |
|  | |
| 0” | |
|  | |
|  | **An identifying mark:**  **Rated Impedance 6ohm**  **Resonant Frequency**  **1000H z**  **Rated Power 10W**  **Max Power 30W**  **Sensitivity(2.83v/1m） 92dB**  **DC resistance 5.4ohm**  **Magnet Neodymium**  **Suggested Crossover >2500Hz** |

